RIOS PRE-PROCESSING PARAMETERS
______________________________

Date and Time: 2026-02-06 22:24
Calculate for Erosion Control: true
Calculate for Phosphorus Retention: true
Calculate for Nitrogen Retention: true
Calculate for Flood Mitigation: true
Calculate for Groundwater Recharge/Baseflow: true
Workspace: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/out/02-PREPROC_RIOS/
Output path: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/out/02-PREPROC_RIOS/
land use/land cover: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/LULC_EU_1.tif
RIOS biophysical coefficient table: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/biophysical_table.csv
DEM: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/DEM_EU_1.tif
rainfall erosivity: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/R_EU_1.tif
erodibility: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/K_EU_1.tif
soil depth: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/Soil_Depth_EU_1.tif
precipitation for wettest month: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/Pcp_EU_1_NOV_11.tif
soil texture: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/SoilIndex_EU_1.tif
annual average precipitation: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/Pcp_EU_1_YEAR_13.tif
actual evapotranspiration: /home/skaphe/Documentos/tnc/modelos/salidas/1019_2431_2026-2-6/WI_1631/in/02-PREPROC_RIOS/ETo_EU_1_YEAR_13.tif
Suffix: EU_1
