RIOS PRE-PROCESSING PARAMETERS
______________________________

Date and Time: 2026-02-06 21:28
Calculate for Erosion Control: true
Calculate for Phosphorus Retention: true
Calculate for Nitrogen Retention: true
Calculate for Flood Mitigation: true
Calculate for Groundwater Recharge/Baseflow: true
Workspace: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/out/02-PREPROC_RIOS/
Output path: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/out/02-PREPROC_RIOS/
land use/land cover: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/LULC_SA_1.tif
RIOS biophysical coefficient table: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/biophysical_table.csv
DEM: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/DEM_SA_1.tif
rainfall erosivity: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/R_SA_1.tif
erodibility: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/K_SA_1.tif
soil depth: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/Soil_Depth_SA_1.tif
precipitation for wettest month: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/Pcp_SA_1_OCT_10.tif
soil texture: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/SoilIndex_SA_1.tif
annual average precipitation: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/Pcp_SA_1_YEAR_13.tif
actual evapotranspiration: /home/skaphe/Documentos/tnc/modelos/salidas/1031_2424_2026-2-6/WI_1630/in/02-PREPROC_RIOS/ETo_SA_1_YEAR_13.tif
Suffix: SA_1
